Alarm Reset  Procedure

Napco  800

 (Enter code) (Keypad will flash what zone went off) count the # of (flashes) (Enter code) again 

850, 900, 1008, 1016   (Enter code) to shut off sounder Press the 9 key (keypad will beep) then (enter code)

2600 & 3000                (Enter code) to shut off sounder Press (reset) key (keypad will beep) then (enter code)
 ----------------------------------------------------------------------------------------------------------------------------------------------------------

MOOSE ZX300 & ZX310

Press (On/Cancel) Button then (enter code)

Moose / Discovery  800, 880, 900, 1080, 1100,

(Enter code) followed by the (* key) to reset & clear all alarms.


Moose 

1100E  Press  button under the word  (silence)   (enter code)   (press)   button under the word     (quit) 

1200     Press
“



“
“



“ 

2000     Press
“



“
“



“

5000     Press
“



“
“



“

---------------------------------------------------------------------------------------------------------------------------------------------------------

Vista  20, 20SE, 20P,

To Silence  Alarm  (ENTER CODE) press the     (OFF) KEY 

To Clear alarm  memory (ENTER CODE)  press (OFF) KEY

--------------------------------------------------------------------------------------------------------------------------------

 Radionics 

(ESC) (PREV)  (ENTER)

DOOR CHIME  

NAPCO  850, 

Press and hold down the (5) key  to turn on or off chime. 

(NOTE) : Chime is only on the entry door zone (1) only  duration of tone is programmable (chip). 

NAPCO  900  THIS PANEL HAS NO CHIME FUNCTION  
NAPCO 1008, 1016  Press and hold down the (5) Key to turn on and off chime. 

CHANGING USER CODES 

MOOSE   300  (8 CODES)   WITH L.C.D. KEYPADS 

 Step 1 
PRESS THE 9 KEY ENTER THE INSTALLER PASS CODE 

 Step 2 
PRESS THE 5 KEY TO PROGRAM USER CODES 

 Step 3 
ENTER THE USER ID THEN PRESS THE (ENTER) KEY

 Step 4 
ENTER THE NEW 4 DIGIT CODE THE KEYPAD WILL BEEP TWICE AND RETURN TO THE

            USER PROMPT.

 REPEAT STEPS #3 & #4  IF MORE THAN ONE CODE CHANGE IS NEEDED IF NOT

 PRESS THE (CLEAR)  KEY TO EXIT PROGRAM  AND RETURN TO READY MODE 

MOOSE  700,     800,      880,      900,     950.

                     (6 CODES)    (8 CODES)       (8 CODES)        (8 CODES)     (8 CODES)

(NOTE: CODE # 1 IS THE MASTER CODE DO NOT CHANGE OR PROGRAM THIS LOCATION)

PRESS AND HOLD  THE (9 KEY) FOR THREE SECONDS KEYPAD WILL BEEP 3 TIMES.

ENTER  MASTER CODE  (KEYPAD WILL BEEP TWO TIMES) ALL LIGHTS WILL FLASH

ENTER CODE LOCATION NUMBER TO BE PROGRAMED  IF CODE LOCATION IS TWO HIT THE (2 KEY) 

FOLLOWED BY THE (# KEY)  ENTER NEW (FOUR DIGIT CODE)  PROGRAM WILL EXIT AUTOMATICALLY.

TEST ALL CODES WHEN DONE.

MOOSE 1100E (17 CODES)

PRESS THE MENU SCROLL KEY THREE TIMES

The MENU scroll KEY  has an ARROW with a  LINE UNDER IT  or the  SECOND KEY UNDER the word LEAVE  

PRESS button under the word (PROGRAM)                         (ENTER MASTER CODE)           

PRESS button under the word  (CONTROL PANEL)   (Display will read ENTER A FUNCTION NUMBER This is the code location )

PRESS  01  for location or  CODE  #1   

PRESS  02  for location or  CODE  #2       up to 17 codes

As the five digit code is entered the Cursor will scroll to the right showing the code that was entered

For a four digit code enter the four digits followed by the zero key.

NOTE: THE SYSTEM WILL AUTO EXIT THE PROGRAM AFTER  EVERY CODE ENTRY   

