SECURE WIRELESS PRODUCTS NOTES

TECH SUPPORT – MIKE- 866-908-8324 
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SWITCHES – WHEN USING MAGNET - LOOP 2

PIR-RESC3 - PROGRAM USING LOOP 2

IF YOU REMOVE BATTERY USE A SCREWDRIVER TO SHORT ACROSS THE RESET JUMPER – LEAVE JUMPER INTACT

· THIS MOTION HAS A CAPACITIVE CIRCUIT THAT WILL ALLOW THE DEVICE TO FUNCTION EVEN AFTER BATTERY HAS BEEN REMOVED ( ( 1 CYCLE OF TRANSMISSION ).

· TO WALK TEST – USE A MAGNET AND SWIPE THE LOWER RIGHT SIDE. DETECGOR WILL GO IN WALK TEST FOR 1 MINUTE (BLUE LED).  PET IMUNE 

· TO PERFORM AN RF TEST OF THE DETECTOR – REMOVE COVER ON THE LOWER RIGHT SIDE OF THE PC BOARD WOU WIL SEE A REED SWITCH WITH A SMALL ORANGE BUTTON TO IT’S LEFT. PRESSING THE SMALL ORANGE BUTTON WILL ACTIVATE AN RF TEST.

· DETECTOR TAKES 2 MINUTES TO STABILIZE ON POWER UP AND AN ALSO 2 MINUTES BETWEEN ALARM TRIPS.`

TROUBLE WITH PIR-REC3 MOTION DETECTOR:

· NOT ENROLLED

· ON ANUAL ENROLLMENT:

· DIFFERENT SERIAL # WHEN ENROLLED

· OR – ASSUMES IDENTITY OF ANOTHER 

· MOTION DETECTOR SERIAL #.

DELETE THE ZONE THAT THE TROUBLESOME DETECTOR

WAS PROGRAMMED FOR. 


-ASSIGN THE DETECTOR TO A DIFFERENT ZONE.

                     ALSO – WHEN INITIALIZING THE DETECTOR… HOLD THE 

                                    TAMPER SWITCH DOWN FOR 20 – 30 SECONDS IF THE

                                    TAMPER DOES NOT TRANSMIT TO THE RECEIVER.

   EV-REC-1 INSTALLATION & PROGRAMMING NOTES

· BENCH TEST 1ST
· WIRE THE RECEIVER TO THE VISTA 20P AS YOU WOULD A KEYPAD

· ASSIGN THE RECEIVER AS DEVICE ID  17 IN THE VISTA 20P

· ASSIGN A USER CODE FOR THE FOB ( ONLY 1 CODE NEEDED FOR BOTH FOBS.

· POWER THE SYSTEM UP 

· OPEN THE COVER ON THE RECEIVER   THERE IS AN LED AND A PUSH BUTTON SWITCH. 

· PUSH THE BUTTON ONCE – RECEIVER SHOULD BE ID AS ADEMCO

· PROGRAMMING THE FOB’S REQUIRES A COUPLE OF STEPS

· AT THE RECEIVER- GIVE THE PROGRAM BUTTON 1 QUICK PUSH….THE LIGHT ON THE RECEIVER SHOUL D TURN  RED
· TAKE 1 KEYFOB & PRESS THE UPPER RIGHT BUTTON (AWAY) ONCE   THE RED LIGHT SHOULD GO OUT

· YOU CAN VERIFY THE FOB WORKS BY PRESSING THE LOWER RIGHT BUTTON (GARAGE DOOR)  THE RELAY ON THE RECEIVER WILL CLICK

· YOU MUST NOW PROGRAM THE KEYFOB TO CORRESPOND WITH THE USER CODE YOU PROGRAMMED FOR THE FOB  (FOLLOW THE INSTALLATION GUIDE FOR PROGRAMMING CODE)

· THE SECOND FOB SHOULD WORK WITHOUT PROGRAMMING…IF NOT DO THE STEPS ABOVE

