VISTA

PROGRAMMING NOTES

1.
5881 ENH Receiver – Leave dip switches @ factory settings 

2.
5816 WIRELESS  - USE  LOOP 1--If using an external switch ( 1078 / 39 etc)




          USE  LOOP 2 -- If using the MAGNET

3.
TROUBLE CODE  107 -  Either a Zone or Relay Trouble

4.
TROUBLE WITH A ZONE – No apparent reason  - device appears OK



Check for DOUBLE resistors.

